**Foundations**

Please see below screenshot of foundation locations as identified in Helix. Majority of locations have foundations already installed (Green).

A map of a city

Description automatically generated

All piles installed and remaining to install are Steel CHS with typically 40-60m between structures. This is subject to change depending on ground conditions experienced on site.

**Mast design**

Spacing can be seen in the screen shot above for foundations.

The majority of the structures are STCs (Single Track Cantilever) in this area, as per images:

A blueprint of a building

Description automatically generated**A pole with a power line attached to it

Description automatically generated**

**A train on the tracks

Description automatically generated**There are also a few TTC (Twin Track Cantilever structures, as per images:

A blueprint of a building

Description automatically generated

**Fencing**

There are plans to upgrade any non-compliant boundary measures to a green powder-coated palisade fence with a minimum height of 1.8m.